2024 Annual Water Quality Report
 Town of Marbleton 
PWS WY5600223
Spanish (Espanol)

Este informe contiene informacion muy importante sobre la calidad de su agua beber. Traduscalo o hable con alguien que lo entienda bien. 
Is my water safe?
We are pleased to present this year's Annual Water Quality Report (Consumer Confidence Report) as required by the Safe Drinking Water Act (SDWA). This report is designed to provide details about where your water comes from, what it contains, and how it compares to standards set by regulatory agencies. This report is a snapshot of last year's water quality. We are committed to providing you with information because informed customers are our best allies.
Do I need to take special precautions?
Some people may be more vulnerable to contaminants in drinking water than the general population. Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. EPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Water Drinking Hotline (800-426-4791). 
Where does my water come from?

Our water consists of six groundwater wells located throughout the Town of Marbleton. Our wells draw water from the Wasatch formation aquifer from depths of 120 feet to nearly 800 feet.
Source water assessment and its availability
Marbleton Town Hall or Town of Marbleton website https://www.marbletonwyo.net/public-works


Why are there contaminants in my drinking water?
Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants. The presence of contaminants does not necessarily indicate that water poses a health risk. More information about contaminants and potential health effects can be obtained by calling the Environmental Protection Agency's (EPA) Safe Drinking Water Hotline (800-426-4791). The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells. As water travels over the surface of the land or through the ground, it dissolves naturally occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity: microbial contaminants, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife; inorganic contaminants, such as salts and metals, which can be naturally occurring or result from urban stormwater runoff, industrial, or domestic wastewater discharges, oil and gas production, mining, or farming; pesticides and herbicides, which may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses; organic Chemical Contaminants, including synthetic and volatile organic chemicals, which are by-products of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, and septic systems; and radioactive contaminants, which can be naturally occurring or be the result of oil and gas production and mining activities. In order to ensure that tap water is safe to drink, EPA prescribes regulations that limit the amount of certain contaminants in water provided by public water systems. Food and Drug Administration (FDA) regulations establish limits for contaminants in bottled water which must provide the same protection for public health.
How can I get involved?
Council meetings on the second Monday of each month starting at 5 pm at Marbleton Town Hall.
Water Conservation Tips
Did you know that the average U.S. household uses approximately 400 gallons of water per day or 100 gallons per person per day? Luckily, there are many low-cost and no-cost ways to conserve water. Small changes can make a big difference - try one today and soon it will become second nature.
· Take short showers - a 5 minute shower uses 4 to 5 gallons of water compared to up to 50 gallons for a bath.
· Shut off water while brushing your teeth, washing your hair and shaving and save up to 500 gallons a month.
· Use a water-efficient showerhead. They're inexpensive, easy to install, and can save you up to 750 gallons a month.
· Run your clothes washer and dishwasher only when they are full. You can save up to 1,000 gallons a month.
· Water plants only when necessary.
· Fix leaky toilets and faucets. Faucet washers are inexpensive and take only a few minutes to replace. To check your toilet for a leak, place a few drops of food coloring in the tank and wait. If it seeps into the toilet bowl without flushing, you have a leak. Fixing it or replacing it with a new, more efficient model can save up to 1,000 gallons a month.
· Adjust sprinklers so only your lawn is watered. Apply water only as fast as the soil can absorb it and during the cooler parts of the day to reduce evaporation.
· Teach your kids about water conservation to ensure a future generation that uses water wisely. Make it a family effort to reduce next month's water bill!
· Visit www.epa.gov/watersense for more information.
Cross Connection Control Survey
The purpose of this survey is to determine whether a cross-connection may exist at your home or business. A cross connection is an unprotected or improper connection to a public water distribution system that may cause contamination or pollution to enter the system. We are responsible for enforcing cross-connection control regulations and insuring that no contaminants can, under any flow conditions, enter the distribution system. If you have any of the devices listed below please contact us so that we can discuss the issue, and if needed, survey your connection and assist you in isolating it if that is necessary. 
· Boiler/ Radiant heater (water heaters not included)
· Underground lawn sprinkler system
· Pool or hot tub (whirlpool tubs not included)
· Additional source(s) of water on the property
· Decorative pond
· Watering trough
Source Water Protection Tips
Protection of drinking water is everyone's responsibility. You can help protect your community's drinking water source in several ways:
· Eliminate excess use of lawn and garden fertilizers and pesticides - they contain hazardous chemicals that can reach your drinking water source.
· Pick up after your pets.
· If you have your own septic system, properly maintain your system to reduce leaching to water sources or consider connecting to a public water system.
· Dispose of chemicals properly; take used motor oil to a recycling center.
· Volunteer in your community. Find a watershed or wellhead protection organization in your community and volunteer to help. If there are no active groups, consider starting one. Use EPA's Adopt Your Watershed to locate groups in your community, or visit the Watershed Information Network's How to Start a Watershed Team.
· Organize a storm drain stenciling project with your local government or water supplier. Stencil a message next to the street drain reminding people "Dump No Waste - Drains to River" or "Protect Your Water." Produce and distribute a flyer for households to remind residents that storm drains dump directly into your local water body.
Monitoring and reporting of compliance data violations
Nitrate and nitrite [measured as Nitrogen]

Infants below the age of six months who drink water containing nitrate and nitrite in excess of the MCL could become seriously ill and, if untreated, may
die. Symptoms include shortness of breath and blue-baby syndrome.

MONITORING, ROUTINE MAJOR 01/01/2024 to12/31/2024 

We failed to test our drinking water for the contaminant and period indicated. Because of this failure, we cannot be sure of the quality of our drinking water during the period indicated.
Significant Deficiencies
Survey Year 2021, SD#I: All openings in Well ID: WL03 - Well #3 must be sealed and watertight.

Survey Year 2021, SD#2: Well ID: WL04 - Well #4 must be fitted with a functioning sanitary seal that is tightly bolted and does not allow contamination to enter the well.

Survey Year 2021, SD#5: The overflow on Tank ID: ST02 - West Tank (200K Gal) must have an air gap present such that the overflow pipe terminates at least three pipe diameters above the ground level at the sewer or storm drain or over a splash pad. The structure underneath the overflow needs to be removed so that water does not pool up in it faster than it can drain, or the overflow needs to be reconfigured to achieve the air gap.

Well ID: WL07 -Well #7

Holes or openings observed in the well or its appurtenances.

To prevent contamination of the well, all openings must be sealed and watertight. The conduit entry point must be made watertight and enter the casing in a proper fitting. Caulking/sealer, due to the possibility of the inclusion of BTEX components, must not be used.

Leaking system components were identified: Multiple components in WLOI well house.

Multiple components in the Well #1 (WLOI) well house were leaking and must be repaired.

Repairs are a work in progress.
Additional Information for Lead
The system inventory does not include lead service lines.
A Lead Service Line inventory was completed by The Town of Marbleton. There were no identified lead service lines, however galvanized and unidentified lines were uncovered. The town of Marbleton is working diligently to replace the lines identified as galvanized and will continue working to identify and replace unknown lines that may contain galvanized or of unknown material.

Information is available at The Town Hall, located at 10700 Highway 189, Big Piney, WY 83113

Lead can cause serious health effects in people of all ages, especially pregnant women, infants, and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. MARBLETON, TOWN OF is responsible for providing high quality drinking water and removing lead pipes but cannot control the variety of materials used in plumbing components in your home. Because lead levels may vary over time, lead exposure is possible even when your tap sampling results do not detect lead at one point in time. You share the responsibility for protecting yourself and your family from the lead in your home plumbing. You can take responsibility by identifying and removing lead materials within your home plumbing and taking steps to reduce your family's risk. Before drinking tap water, flush your pipes for several minutes by running your tap, taking a shower, doing laundry or a load of dishes. Use only cold water for drinking, cooking, and making baby formula. Boiling water does not remove lead from water. If you have a lead service line or galvanized requiring replacement service line, you may need to flush your pipes for a longer period. You can also use a filter certified by an American National Standards Institute accredited certifier to reduce lead in drinking water. If you are concerned about lead in your water and wish to have your water tested, contact MARBLETON, TOWN OF (Public Watersystem Id: WY5600223) by calling 307-276-3815 or emailing marbletonwatersewer@gmail.com. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at http://www.epa.gov/safewater/lead.


Water Quality Data Table
In order to ensure that tap water is safe to drink, EPA prescribes regulations which limit the amount of contaminants in water provided by public water systems. The table below lists all of the drinking water contaminants that we detected during the calendar year of this report. Although many more contaminants were tested, only those substances listed below were found in your water. All sources of drinking water contain some naturally occurring contaminants. At low levels, these substances are generally not harmful in our drinking water. Removing all contaminants would be extremely expensive, and in most cases, would not provide increased protection of public health. A few naturally occurring minerals may actually improve the taste of drinking water and have nutritional value at low levels. Unless otherwise noted, the data presented in this table is from testing done in the calendar year of the report. The EPA or the State requires us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not vary significantly from year to year, or the system is not considered vulnerable to this type of contamination. As such, some of our data, though representative, may be more than one year old. In this table you will find terms and abbreviations that might not be familiar to you. To help you better understand these terms, we have provided the definitions below the table.

	Contaminants
	MCLG
or
MRDLG
	MCL,
TT, or
MRDL
	Detect In
Your Water
	Range
	Sample
Date
	Violation
	Typical Source

	
	
	
	
	Low
	High
	
	
	

	Inorganic Contaminants

	Fluoride (ppm)
	4
	4
	2.4
	1.8
	2.4
	2024
	No
	Erosion of natural deposits; Water additive which promotes strong teeth; Discharge from fertilizer and aluminum factories

	Nitrate [measured as Nitrogen] (ppm)
	10
	10
	0.4
	00
	0.4
	2024
	No
	Runoff from fertilizer use; Leaching from septic tanks, sewage; Erosion of natural deposits

	Thallium (ppb)
	0.5
	2
	0.5
	00
	0.5
	2021
	No
	Discharge from electronics, glass, and Leaching from ore-processing sites; drug factories

	Radioactive Contaminants

	Alpha emitters (pCi/L)
	00
	15
	5.6
	0-8.4
	5.6
	2021
	No
	Erosion of natural deposits

	Radium (combined 226/228) (pCi/L)
	00
	5
	1.5
	0.6
	1.5
	2021
	No
	Erosion of natural deposits

	Uranium (ug/L)
	00
	30
	2.4
	0.5
	2.4
	2021
	No
	Erosion of natural deposits



	Contaminants
	MCLG
	AL
	90th Percentile
	Range
	# Samples
Exceeding AL
	Sample
Date
	Exceeds AL
	Typical Source

	
	
	
	
	Low
	High
	
	
	
	

	Inorganic Contaminants
	
	

	Copper - action level at consumer taps (ppm)
	1.3
	1.3
	0.06
	00
	0.15
	0
	2024
	No
	Corrosion of household plumbing systems; Erosion of natural deposits

	Lead - action level at consumer taps (ppb)
	00
	15
	2
	00
	9
	0
	2024
	No
	Corrosion of household plumbing systems; Erosion of natural deposits



	Violations and Exceedances




	Unit Descriptions

	Term
	Definition

	ug/L
	ug/L : Number of micrograms of substance in one liter of water

	ppm
	ppm: parts per million, or milligrams per liter (mg/L)

	ppb
	ppb: parts per billion, or micrograms per liter (µg/L)

	pCi/L
	pCi/L: picocuries per liter (a measure of radioactivity)

	NA
	NA: not applicable

	ND
	ND: Not detected

	NR
	NR: Monitoring not required, but recommended.



	Important Drinking Water Definitions

	Term
	Definition

	MCLG
	MCLG: Maximum Contaminant Level Goal: The level of a contaminant in drinking water below which there is no known or expected risk to health. MCLGs allow for a margin of safety.

	MCL
	MCL: Maximum Contaminant Level: The highest level of a contaminant that is allowed in drinking water. MCLs are set as close to the MCLGs as feasible using the best available treatment technology.

	TT
	TT: Treatment Technique: A required process intended to reduce the level of a contaminant in drinking water.

	AL
	AL: Action Level: The concentration of a contaminant which, if exceeded, triggers treatment or other requirements which a water system must follow.

	Variances and Exemptions
	Variances and Exemptions: State or EPA permission not to meet an MCL or a treatment technique under certain conditions.

	MRDLG
	MRDLG: Maximum residual disinfection level goal. The level of a drinking water disinfectant below which there is no known or expected risk to health. MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.

	MRDL
	MRDL: Maximum residual disinfectant level. The highest level of a disinfectant allowed in drinking water. There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.

	MNR
	MNR: Monitored Not Regulated

	MPL
	MPL: State Assigned Maximum Permissible Level

	90th Percentile
	Compliance with the lead and copper action levels is based on the 90th percentile lead and copper levels. This means that the concentration of lead and copper must be less than or equal to the action level in at least 90% of the samples collected.




	TT Violation
	Explanation
	Length
	Explanation and Comment
	Health Effects Language

	Ground Water Rule violations
	Failure to address significant deficiency
	Violation Start Date: 10/17/2024
Violation End Date: 2024
	Contact Josh Rogers at 307-276-3815 or email marbletontown@hotmail.com for more information.
	Inadequately treated water may contain disease-causing organisms. These organisms include bacteria, viruses, and parasites, which can cause symptoms such as nausea, cramps, diarrhea, and associated headaches.



	For more information please contact:


Contact Name: ROGERS, JOSHUA
Address: 10700 Highway 189
MARBLETON, WY 83113
Phone: 307-276-3815
